
Crumar Sorrento - update CTRL v.1.0.1

How to update:
1. You need a Windows x64 computer (Mac users please use a Windows computer)
2. Connect Sorrento to your computer using a USB cable
3. Turn on Sorrento
4. Launch updater App
5. Click connect and wait until the update completes
6. You can verify firmware version on the OLED Display when Sorrento is powered on.

New in this release:
- Fixed bug with sporadical stuck notes while using a 50K expression pedal
- Sustain Pedal no longer sends CC#64 twice when SEND CC option is on
- Added Panic! function that can be used by holding down the minus (-) button while OLED is off
- Keyclick and Perc.Vol knobs are properly scanned when they are set to zero at bootup
- Changing global tuning now also works on the bass pedal synth
- In spinet or transistor mode, recalling an upper preset no longer turns off first percussion LED

For more information, please visit www.crumar.it

